# NCC Spoke RA Module

This module allows management of NCC Spokes backed by Router Appliances. Network virtual appliances used as router appliances allow to connect an external network to Google Cloud by using a SD-WAN router or another appliance with BGP capabilities (_site-to-cloud_ connectivity). It is also possible to enable site-to-site data transfer, although this feature is not available in all regions, particularly not in EMEA.

The module manages a hub (optionally), a spoke, and the corresponding Cloud Router and BGP sessions to the router appliance(s).

## Examples

### Simple hub & spoke

```hcl
module "spoke-ra" {
  source     = "./fabric/modules/ncc-spoke-ra"
  hub        = { create = true, name = "ncc-hub" }
  name       = "spoke-ra"
  project_id = var.project_id
  region     = var.region
  router_appliances = [
    {
      internal_ip  = module.compute-vm-primary-b.internal_ip
      vm_self_link = module.compute-vm-primary-b.self_link
    }
  ]
  router_config = {
    asn           = 65000
    ip_interface0 = "10.0.16.14"
    ip_interface1 = "10.0.16.15"
    peer_asn      = 65001
  }
  vpc_config = {
    network_name     = var.vpc.self_link
    subnet_self_link = var.subnet.self_link
  }
}
# tftest modules=5 resources=11 fixtures=fixtures/compute-vm-nva.tf e2e
```

### Two spokes

```hcl
resource "google_network_connectivity_hub" "default" {
  name        = "Hub"
  description = "Hub"
  project     = var.project_id
}

module "spoke-ra-a" {
  source     = "./fabric/modules/ncc-spoke-ra"
  hub        = { id = google_network_connectivity_hub.default.id }
  name       = "spoke-ra-a"
  project_id = var.project_id
  region     = var.regions.primary
  router_appliances = [
    {
      internal_ip  = module.compute-vm-primary-b.internal_ip
      vm_self_link = module.compute-vm-primary-b.self_link
    }
  ]
  router_config = {
    asn           = 65000
    ip_interface0 = "10.0.16.14"
    ip_interface1 = "10.0.16.15"
    peer_asn      = 65001
  }
  vpc_config = {
    network_name     = var.vpc.self_link
    subnet_self_link = var.subnets.primary.self_link
  }
}

module "spoke-ra-b" {
  source     = "./fabric/modules/ncc-spoke-ra"
  hub        = { id = google_network_connectivity_hub.default.id }
  name       = "spoke-ra-b"
  project_id = var.project_id
  region     = var.regions.secondary
  router_appliances = [
    {
      internal_ip  = module.compute-vm-secondary-b.internal_ip
      vm_self_link = module.compute-vm-secondary-b.self_link
    }
  ]
  router_config = {
    asn           = 65000
    ip_interface0 = "10.1.16.14"
    ip_interface1 = "10.1.16.15"
    peer_asn      = 65002
  }
  vpc_config = {
    network_name     = var.vpc.self_link
    subnet_self_link = var.subnets.secondary.self_link
  }
}
# tftest modules=6 resources=17 fixtures=fixtures/compute-vm-nva.tf e2e
```

### Spoke with load-balanced router appliances

```hcl
resource "google_network_connectivity_hub" "default" {
  name        = "Hub"
  description = "Hub"
  project     = var.project_id
}

module "spoke-ra" {
  source     = "./fabric/modules/ncc-spoke-ra"
  hub        = { id = google_network_connectivity_hub.default.id }
  name       = "spoke-ra"
  project_id = var.project_id
  region     = var.region
  router_appliances = [
    {
      internal_ip  = module.compute-vm-primary-b.internal_ip
      vm_self_link = module.compute-vm-primary-b.self_link
    },
    {
      internal_ip  = module.compute-vm-primary-c.internal_ip
      vm_self_link = module.compute-vm-primary-c.self_link
    }
  ]
  router_config = {
    asn = 65000
    custom_advertise = {
      all_subnets = true
      ip_ranges = {
        "10.10.0.0/24" = "peered-vpc"
      }
    }
    ip_interface0 = "10.0.16.14"
    ip_interface1 = "10.0.16.15"
    peer_asn      = 65001
  }
  vpc_config = {
    network_name     = var.vpc.self_link
    subnet_self_link = var.subnet.self_link
  }
}
# tftest modules=5 resources=13 fixtures=fixtures/compute-vm-nva.tf e2e
```
<!-- BEGIN TFDOC -->
## Variables

| name | description | type | required | default |
|---|---|:---:|:---:|:---:|
| [hub](variables.tf#L23) | The NCC hub. You should either provide an existing hub id or a hub name if create is true. | <code>object&#40;&#123;&#8230;&#125;&#41;</code> | ✓ |  |
| [name](variables.tf#L37) | The name of the NCC spoke. | <code>string</code> | ✓ |  |
| [project_id](variables.tf#L42) | The ID of the project where the NCC hub & spokes will be created. | <code>string</code> | ✓ |  |
| [region](variables.tf#L47) | Region where the spoke is located. | <code>string</code> | ✓ |  |
| [router_appliances](variables.tf#L52) | List of router appliances this spoke is associated with. | <code>list&#40;object&#40;&#123;&#8230;&#125;&#41;&#41;</code> | ✓ |  |
| [router_config](variables.tf#L60) | Configuration of the Cloud Router. | <code>object&#40;&#123;&#8230;&#125;&#41;</code> | ✓ |  |
| [vpc_config](variables.tf#L76) | Network and subnetwork for the CR interfaces. | <code>object&#40;&#123;&#8230;&#125;&#41;</code> | ✓ |  |
| [data_transfer](variables.tf#L17) | Site-to-site data transfer feature, available only in some regions. | <code>bool</code> |  | <code>false</code> |

## Outputs

| name | description | sensitive |
|---|---|:---:|
| [hub](outputs.tf#L17) | NCC hub resource (only if auto-created). |  |
| [id](outputs.tf#L22) | Fully qualified hub id. |  |
| [router](outputs.tf#L27) | Cloud Router resource. |  |
| [spoke_ra](outputs.tf#L32) | NCC spoke resource. |  |

## Fixtures

- [compute-vm-nva.tf](../../tests/fixtures/compute-vm-nva.tf)
<!-- END TFDOC -->
